(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "74xx:74HC138"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 13.97 0)
			)
			(property "Value" "74HC138"
				(at 2.54 -11.43 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc238.pdf"
				(at 0 0 0)
			)
			(property "Description" "3-to-8 line decoder/multiplexer inverting, DIP-16/SOIC-16/SSOP-16"
				(at 0 0 0)
			)
			(property "ki_keywords" "demux"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*"
				(at 0 0 0)
			)
			(symbol "74HC138_0_1"
				(rectangle
					(start -7.62 12.7)
					(end 7.62 -10.16)
					(fill
						(type background)
					)
				)
			)
			(symbol "74HC138_1_1"
				(pin input line
					(at -10.16 10.16 0)
					(length 2.54)
					(name "A0")
					(number "1")
				)
				(pin input line
					(at -10.16 7.62 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at -10.16 5.08 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin input line
					(at -10.16 -2.54 0)
					(length 2.54)
					(name "~{E0}")
					(number "4")
				)
				(pin input line
					(at -10.16 -5.08 0)
					(length 2.54)
					(name "~{E1}")
					(number "5")
				)
				(pin input line
					(at -10.16 -7.62 0)
					(length 2.54)
					(name "E2")
					(number "6")
				)
				(pin power_in line
					(at 0 15.24 270)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
				(pin power_in line
					(at 0 -12.7 90)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin output line
					(at 10.16 10.16 180)
					(length 2.54)
					(name "~{Y0}")
					(number "15")
				)
				(pin output line
					(at 10.16 7.62 180)
					(length 2.54)
					(name "~{Y1}")
					(number "14")
				)
				(pin output line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "~{Y2}")
					(number "13")
				)
				(pin output line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "~{Y3}")
					(number "12")
				)
				(pin output line
					(at 10.16 0 180)
					(length 2.54)
					(name "~{Y4}")
					(number "11")
				)
				(pin output line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "~{Y5}")
					(number "10")
				)
				(pin output line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "~{Y6}")
					(number "9")
				)
				(pin output line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "~{Y7}")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
		(symbol "74xx:74HC374"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 16.51 0)
			)
			(property "Value" "74HC374"
				(at -7.62 -16.51 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hct374.pdf"
				(at 0 0 0)
			)
			(property "Description" "8-bit Register, 3-state outputs"
				(at 0 0 0)
			)
			(property "ki_keywords" "HCMOS DFF DFF8 REG 3State"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP?20* SOIC?20* SO?20*"
				(at 0 0 0)
			)
			(symbol "74HC374_1_0"
				(pin input line
					(at -12.7 12.7 0)
					(length 5.08)
					(name "D0")
					(number "3")
				)
				(pin input line
					(at -12.7 10.16 0)
					(length 5.08)
					(name "D1")
					(number "4")
				)
				(pin input line
					(at -12.7 7.62 0)
					(length 5.08)
					(name "D2")
					(number "7")
				)
				(pin input line
					(at -12.7 5.08 0)
					(length 5.08)
					(name "D3")
					(number "8")
				)
				(pin input line
					(at -12.7 2.54 0)
					(length 5.08)
					(name "D4")
					(number "13")
				)
				(pin input line
					(at -12.7 0 0)
					(length 5.08)
					(name "D5")
					(number "14")
				)
				(pin input line
					(at -12.7 -2.54 0)
					(length 5.08)
					(name "D6")
					(number "17")
				)
				(pin input line
					(at -12.7 -5.08 0)
					(length 5.08)
					(name "D7")
					(number "18")
				)
				(pin input clock
					(at -12.7 -10.16 0)
					(length 5.08)
					(name "Cp")
					(number "11")
				)
				(pin input inverted
					(at -12.7 -12.7 0)
					(length 5.08)
					(name "OE")
					(number "1")
				)
				(pin power_in line
					(at 0 20.32 270)
					(length 5.08)
					(name "VCC")
					(number "20")
				)
				(pin power_in line
					(at 0 -20.32 90)
					(length 5.08)
					(name "GND")
					(number "10")
				)
				(pin tri_state line
					(at 12.7 12.7 180)
					(length 5.08)
					(name "O0")
					(number "2")
				)
				(pin tri_state line
					(at 12.7 10.16 180)
					(length 5.08)
					(name "O1")
					(number "5")
				)
				(pin tri_state line
					(at 12.7 7.62 180)
					(length 5.08)
					(name "O2")
					(number "6")
				)
				(pin tri_state line
					(at 12.7 5.08 180)
					(length 5.08)
					(name "O3")
					(number "9")
				)
				(pin tri_state line
					(at 12.7 2.54 180)
					(length 5.08)
					(name "O4")
					(number "12")
				)
				(pin tri_state line
					(at 12.7 0 180)
					(length 5.08)
					(name "O5")
					(number "15")
				)
				(pin tri_state line
					(at 12.7 -2.54 180)
					(length 5.08)
					(name "O6")
					(number "16")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "O7")
					(number "19")
				)
			)
			(symbol "74HC374_1_1"
				(rectangle
					(start -7.62 15.24)
					(end 7.62 -15.24)
					(fill
						(type background)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "CPU:Z84C00xxP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -9.652 34.798 0)
			)
			(property "Value" "Z84C00xxP"
				(at 3.81 34.798 0)
			)
			(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
				(at 0 -42.418 0)
			)
			(property "Datasheet" "https://archive.org/details/zilog-z-8400"
				(at 0 -40.132 0)
			)
			(property "Description" "8-bit General Purpose Microprocessor, 8-bit data bus, 16-bit address bus, up to 6.17 / 8 / 10 / 20 MHz, CMOS version, DIP-40 (600 mil)"
				(at 0 -38.1 0)
			)
			(property "ki_keywords" "Zilog Z80-CPU 8080A Z84C0006 Z84C0008 Z84C0010 Z84C0020"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W15.24*"
				(at 0 0 0)
			)
			(symbol "Z84C00xxP_0_1"
				(rectangle
					(start -10.16 33.02)
					(end 10.16 -33.02)
					(fill
						(type background)
					)
				)
			)
			(symbol "Z84C00xxP_1_1"
				(pin input clock
					(at -12.7 30.48 0)
					(length 2.54)
					(name "CLK")
					(number "6")
				)
				(pin output line
					(at -12.7 22.86 0)
					(length 2.54)
					(name "~{M1}")
					(number "27")
				)
				(pin tri_state line
					(at -12.7 17.78 0)
					(length 2.54)
					(name "~{MREQ}")
					(number "19")
				)
				(pin tri_state line
					(at -12.7 15.24 0)
					(length 2.54)
					(name "~{IORQ}")
					(number "20")
				)
				(pin tri_state line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "~{RD}")
					(number "21")
				)
				(pin tri_state line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "~{WR}")
					(number "22")
				)
				(pin output line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "~{RFSH}")
					(number "28")
				)
				(pin input line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "~{BUSREQ}")
					(number "25")
				)
				(pin output line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "~{BUSACK}")
					(number "23")
				)
				(pin input line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "~{INT}")
					(number "16")
				)
				(pin input line
					(at -12.7 -15.24 0)
					(length 2.54)
					(name "~{NMI}")
					(number "17")
				)
				(pin output line
					(at -12.7 -20.32 0)
					(length 2.54)
					(name "~{HALT}")
					(number "18")
				)
				(pin input line
					(at -12.7 -22.86 0)
					(length 2.54)
					(name "~{WAIT}")
					(number "24")
				)
				(pin input line
					(at -12.7 -27.94 0)
					(length 2.54)
					(name "~{RESET}")
					(number "26")
				)
				(pin power_in line
					(at 0 35.56 270)
					(length 2.54)
					(name "V_{CC}")
					(number "11")
				)
				(pin power_in line
					(at 0 -35.56 90)
					(length 2.54)
					(name "GND")
					(number "29")
				)
				(pin tri_state line
					(at 12.7 30.48 180)
					(length 2.54)
					(name "A_{0}")
					(number "30")
				)
				(pin tri_state line
					(at 12.7 27.94 180)
					(length 2.54)
					(name "A_{1}")
					(number "31")
				)
				(pin tri_state line
					(at 12.7 25.4 180)
					(length 2.54)
					(name "A_{2}")
					(number "32")
				)
				(pin tri_state line
					(at 12.7 22.86 180)
					(length 2.54)
					(name "A_{3}")
					(number "33")
				)
				(pin tri_state line
					(at 12.7 20.32 180)
					(length 2.54)
					(name "A_{4}")
					(number "34")
				)
				(pin tri_state line
					(at 12.7 17.78 180)
					(length 2.54)
					(name "A_{5}")
					(number "35")
				)
				(pin tri_state line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "A_{6}")
					(number "36")
				)
				(pin tri_state line
					(at 12.7 12.7 180)
					(length 2.54)
					(name "A_{7}")
					(number "37")
				)
				(pin tri_state line
					(at 12.7 10.16 180)
					(length 2.54)
					(name "A_{8}")
					(number "38")
				)
				(pin tri_state line
					(at 12.7 7.62 180)
					(length 2.54)
					(name "A_{9}")
					(number "39")
				)
				(pin tri_state line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "A_{10}")
					(number "40")
				)
				(pin tri_state line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "A_{11}")
					(number "1")
				)
				(pin tri_state line
					(at 12.7 0 180)
					(length 2.54)
					(name "A_{12}")
					(number "2")
				)
				(pin tri_state line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "A_{13}")
					(number "3")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "A_{14}")
					(number "4")
				)
				(pin tri_state line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "A_{15}")
					(number "5")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "D_{0}")
					(number "14")
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "D_{1}")
					(number "15")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "D_{2}")
					(number "12")
				)
				(pin bidirectional line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "D_{3}")
					(number "8")
				)
				(pin bidirectional line
					(at 12.7 -22.86 180)
					(length 2.54)
					(name "D_{4}")
					(number "7")
				)
				(pin bidirectional line
					(at 12.7 -25.4 180)
					(length 2.54)
					(name "D_{5}")
					(number "9")
				)
				(pin bidirectional line
					(at 12.7 -27.94 180)
					(length 2.54)
					(name "D_{6}")
					(number "10")
				)
				(pin bidirectional line
					(at 12.7 -30.48 180)
					(length 2.54)
					(name "D_{7}")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Simulation_SPICE:NPN"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at -2.54 7.62 0)
			)
			(property "Value" "NPN"
				(at -2.54 5.08 0)
			)
			(property "Footprint" ""
				(at 63.5 0 0)
			)
			(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
				(at 63.5 0 0)
			)
			(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
				(at 0 0 0)
			)
			(property "Sim.Device" "NPN"
				(at 0 0 0)
			)
			(property "Sim.Type" "GUMMELPOON"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=C 2=B 3=E"
				(at 0 0 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "NPN_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 0.635 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 1.905) (xy 0.635 -1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 0.635) (xy 2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 -0.635) (xy 2.54 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.778) (xy 1.778 -1.27) (xy 2.286 -2.286) (xy 1.27 -1.778) (xy 1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 -1.27) (xy 2.794 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 -1.27) (xy 2.794 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "NPN_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin open_collector line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "C")
					(number "1")
				)
				(pin open_emitter line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "E")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 267.97 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 260.35 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 267.97 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 114.3)
		(diameter 0)
		(color 0 0 0 1)
	)
	(bus
		(pts
			(xy 62.23 16.51) (xy 267.97 16.51)
		)
	)
	(wire
		(pts
			(xy 207.01 83.82) (xy 123.19 83.82)
		)
	)
	(wire
		(pts
			(xy 260.35 128.27) (xy 260.35 60.96)
		)
	)
	(wire
		(pts
			(xy 191.77 16.51) (xy 191.77 53.34)
		)
	)
	(wire
		(pts
			(xy 241.3 50.8) (xy 229.87 50.8)
		)
	)
	(wire
		(pts
			(xy 207.01 91.44) (xy 123.19 91.44)
		)
	)
	(wire
		(pts
			(xy 97.79 53.34) (xy 76.2 53.34)
		)
	)
	(wire
		(pts
			(xy 76.2 53.34) (xy 76.2 27.94)
		)
	)
	(wire
		(pts
			(xy 250.19 114.3) (xy 250.19 162.56)
		)
	)
	(wire
		(pts
			(xy 194.31 128.27) (xy 260.35 128.27)
		)
	)
	(wire
		(pts
			(xy 207.01 93.98) (xy 123.19 93.98)
		)
	)
	(wire
		(pts
			(xy 267.97 16.51) (xy 267.97 33.02)
		)
	)
	(wire
		(pts
			(xy 110.49 16.51) (xy 110.49 33.02)
		)
	)
	(bus
		(pts
			(xy 64.77 162.56) (xy 264.16 162.56)
		)
	)
	(wire
		(pts
			(xy 76.2 27.94) (xy 172.72 27.94)
		)
	)
	(wire
		(pts
			(xy 97.79 58.42) (xy 74.93 58.42)
		)
	)
	(wire
		(pts
			(xy 207.01 81.28) (xy 123.19 81.28)
		)
	)
	(wire
		(pts
			(xy 172.72 27.94) (xy 172.72 55.88)
		)
	)
	(wire
		(pts
			(xy 194.31 104.14) (xy 194.31 128.27)
		)
	)
	(wire
		(pts
			(xy 74.93 25.4) (xy 173.99 25.4)
		)
	)
	(wire
		(pts
			(xy 207.01 88.9) (xy 123.19 88.9)
		)
	)
	(wire
		(pts
			(xy 173.99 50.8) (xy 209.55 50.8)
		)
	)
	(wire
		(pts
			(xy 267.97 60.96) (xy 267.97 73.66)
		)
	)
	(wire
		(pts
			(xy 248.92 50.8) (xy 255.27 50.8)
		)
	)
	(wire
		(pts
			(xy 207.01 99.06) (xy 123.19 99.06)
		)
	)
	(wire
		(pts
			(xy 207.01 96.52) (xy 123.19 96.52)
		)
	)
	(wire
		(pts
			(xy 173.99 25.4) (xy 173.99 50.8)
		)
	)
	(wire
		(pts
			(xy 219.71 114.3) (xy 250.19 114.3)
		)
	)
	(wire
		(pts
			(xy 172.72 55.88) (xy 209.55 55.88)
		)
	)
	(wire
		(pts
			(xy 123.19 43.18) (xy 209.55 43.18)
		)
	)
	(wire
		(pts
			(xy 110.49 104.14) (xy 110.49 162.56)
		)
	)
	(wire
		(pts
			(xy 123.19 40.64) (xy 209.55 40.64)
		)
	)
	(wire
		(pts
			(xy 219.71 73.66) (xy 267.97 73.66)
		)
	)
	(wire
		(pts
			(xy 267.97 33.02) (xy 267.97 60.96)
		)
	)
	(wire
		(pts
			(xy 74.93 58.42) (xy 74.93 25.4)
		)
	)
	(wire
		(pts
			(xy 219.71 60.96) (xy 250.19 60.96)
		)
	)
	(wire
		(pts
			(xy 219.71 33.02) (xy 267.97 33.02)
		)
	)
	(wire
		(pts
			(xy 209.55 53.34) (xy 191.77 53.34)
		)
	)
	(wire
		(pts
			(xy 207.01 104.14) (xy 194.31 104.14)
		)
	)
	(wire
		(pts
			(xy 250.19 60.96) (xy 250.19 114.3)
		)
	)
	(wire
		(pts
			(xy 255.27 50.8) (xy 255.27 53.34)
		)
	)
	(wire
		(pts
			(xy 207.01 86.36) (xy 123.19 86.36)
		)
	)
	(wire
		(pts
			(xy 123.19 38.1) (xy 209.55 38.1)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 62.23 16.51 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 66.04 16.51 0)
		)
		(property "Value" "+5V"
			(at 58.42 16.5099 90)
		)
		(property "Footprint" ""
			(at 62.23 16.51 0)
		)
		(property "Datasheet" ""
			(at 62.23 16.51 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 62.23 16.51 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74HC138")
		(at 219.71 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 221.8533 30.48 0)
		)
		(property "Value" "74HC138"
			(at 221.8533 33.02 0)
		)
		(property "Footprint" ""
			(at 219.71 48.26 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc238.pdf"
			(at 219.71 48.26 0)
		)
		(property "Description" "3-to-8 line decoder/multiplexer inverting, DIP-16/SOIC-16/SSOP-16"
			(at 219.71 48.26 0)
		)
		(pin "7")
		(pin "9")
		(pin "8")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "12")
		(pin "11")
		(pin "6")
		(pin "5")
		(pin "10")
		(pin "4")
		(pin "3")
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 64.77 162.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 64.77 168.91 0)
		)
		(property "Value" "GND"
			(at 64.77 167.64 0)
		)
		(property "Footprint" ""
			(at 64.77 162.56 0)
		)
		(property "Datasheet" ""
			(at 64.77 162.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 64.77 162.56 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "CPU:Z84C00xxP")
		(at 110.49 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 112.6333 30.48 0)
		)
		(property "Value" "Z84C00xxP"
			(at 112.6333 33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 110.49 110.998 0)
		)
		(property "Datasheet" "https://archive.org/details/zilog-z-8400"
			(at 110.49 108.712 0)
		)
		(property "Description" "8-bit General Purpose Microprocessor, 8-bit data bus, 16-bit address bus, up to 6.17 / 8 / 10 / 20 MHz, CMOS version, DIP-40 (600 mil)"
			(at 110.49 106.68 0)
		)
		(pin "18")
		(pin "24")
		(pin "16")
		(pin "29")
		(pin "17")
		(pin "30")
		(pin "26")
		(pin "33")
		(pin "11")
		(pin "34")
		(pin "31")
		(pin "37")
		(pin "32")
		(pin "3")
		(pin "35")
		(pin "2")
		(pin "36")
		(pin "1")
		(pin "23")
		(pin "38")
		(pin "40")
		(pin "39")
		(pin "4")
		(pin "5")
		(pin "25")
		(pin "20")
		(pin "28")
		(pin "27")
		(pin "6")
		(pin "21")
		(pin "19")
		(pin "22")
		(pin "12")
		(pin "13")
		(pin "10")
		(pin "9")
		(pin "7")
		(pin "8")
		(pin "14")
		(pin "15")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 245.11 50.8 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 245.11 44.45 90)
		)
		(property "Value" "10K"
			(at 245.11 46.99 90)
		)
		(property "Footprint" ""
			(at 245.11 52.578 90)
		)
		(property "Datasheet" "~"
			(at 245.11 50.8 0)
		)
		(property "Description" "Resistor"
			(at 245.11 50.8 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xx:74HC374")
		(at 219.71 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 221.8533 73.66 0)
		)
		(property "Value" "74HC374"
			(at 221.8533 76.2 0)
		)
		(property "Footprint" ""
			(at 219.71 93.98 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd74hct374.pdf"
			(at 219.71 93.98 0)
		)
		(property "Description" "8-bit Register, 3-state outputs"
			(at 219.71 93.98 0)
		)
		(pin "7")
		(pin "3")
		(pin "4")
		(pin "2")
		(pin "12")
		(pin "5")
		(pin "6")
		(pin "15")
		(pin "9")
		(pin "19")
		(pin "16")
		(pin "13")
		(pin "8")
		(pin "20")
		(pin "11")
		(pin "1")
		(pin "10")
		(pin "17")
		(pin "14")
		(pin "18")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 264.16 60.96 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 264.16 54.61 90)
		)
		(property "Value" "10K"
			(at 264.16 57.15 90)
		)
		(property "Footprint" ""
			(at 264.16 62.738 90)
		)
		(property "Datasheet" "~"
			(at 264.16 60.96 0)
		)
		(property "Description" "Resistor"
			(at 264.16 60.96 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Stoplight"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Simulation_SPICE:NPN")
		(at 255.27 58.42 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q1"
			(at 255.27 64.77 90)
		)
		(property "Value" "NPN"
			(at 255.27 67.31 90)
		)
		(property "Footprint" ""
			(at 255.27 121.92 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 255.27 121.92 0)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 255.27 58.42 0)
		)
		(property "Sim.Device" "NPN"
			(at 255.27 58.42 0)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 255.27 58.42 0)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 255.27 58.42 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
